EXISTING SEWAGE AND/OR PRIVATE WATER SYSTEM EVALUATION APPLICATION

TEST REQUESTED: \_\_\_SEWAGE($150) \_\_\_ WATER($100) ADDITIONAL DATA REQUESTED \_\_\_LEAD \_\_\_NITRATE

PROPERTY ADDRESS:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Parcel ID\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

897 East Iron Avenue

Dover, Ohio 44622

# TUSCARAWAS COUNTY GENERAL HEALTH DISTRICT

Phone (330) 343- 5555

Fax (330) 343-1601

Email director@tchdnow.org

Web site www.tchdnow.org

CITY\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ STATE\_\_\_\_\_\_\_\_\_\_\_\_\_ TOWNSHIP\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* OWNER’S NAME\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ OWNER’S PHONE\_\_\_\_\_\_\_\_\_\_\_\_\_\_

MAILING ADDRESS:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

OWNER’S EMAIL\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* BUYER’S NAME\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ BUYERS PHONE\_\_\_\_\_\_\_\_\_\_\_\_\_

MAILING ADDRESS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

BUYER’S EMAIL\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**PLACE A CHECK NEXT TO THE PERSON RESPONSIBLE FOR PROVIDING ACCESS TO THE PROPERTY**

YEAR OF HOME CONSTRUCTION\_\_\_\_\_\_\_\_\_\_\_\_\_ NUMBER OF BEDROOMS\_\_\_\_\_\_

PROPERTY HAS: \_\_\_\_HOME SEWAGE TREATMENT SYSTEM \_\_\_SEWER

 \_\_\_\_\_PRIVATE WATER (WELL, CISTERN) \_\_\_\_PUBLIC WATER

|  |
| --- |
| THE OPINION GIVEN IS RENDERED WITHOUT KNOWLEDGE OF SOME OF THE INDIVIDUAL PARTS OF THE SYSTEM BEING EVAUATED AND ONLY APPLIES TO THE DATE AND TIME THE OPINION IS MADE. THEREFORM, THIS OPINION DOES NOT GAURANTEE THE FUTURE PERFORMANCE OF THE SYSTEM(S) BEING EVALUATED. THE WATER TEST DO NOT ASSESS THE CHEMICAL QUALITYOF THE WATER, OTHER THAN WHAT IS LISTED |

The fee for inspection must accompany this form. Forms submitted without fee will be returned.

In order to have a complete inspection of the Sewage Treatment system the following must occur:

1. The septic tank lids and all D-boxes must be easily accessible.
2. The septic tank(s) must not be pumped within 60 days of the inspection
3. Water and power must be available to the property to perform the test

In order to have a complete inspection of the Private Water System the following must occur:

1. Power must be on and the system must be operable
2. If the water system has been chlorinated prior to sampling, the water system must be free of chlorine for at least 48 hours prior to obtaining the sample.
3. If sampling include lead testing , NO water may be run in the house for at least 8 hours prior to obtaining the lead sample.